## Reporting + (07-10 10:33:27.200)
## Camera Hal Service (camerahalserver pid:920 32BIT) user-build ## fd:10 options(#0) =
  ICameraProviderCallback 0xa7e4c780 {.pid = -1, .ptr = 0, .arch = IS_32BIT}
## Camera device manager (since 07-10 10:22:17.180) ##
  Physical Devices: # 3
    [00] -> orientation(wanted/setup)=( 90/90 ) BACK  hasFlashUnit:1 SENSOR_DRVNAME_MOT_ELLIS_HI1336_MIPI_RAW [PhysEnumDevice:0xa79577c0]
    [01] -> orientation(wanted/setup)=(270/270) FRONT hasFlashUnit:0 SENSOR_DRVNAME_MOT_ELLIS_SC500CS_MIPI_RAW [PhysEnumDevice:0xa7957820]
    [02] -> orientation(wanted/setup)=(270/90 ) BACK  hasFlashUnit:0 SENSOR_DRVNAME_MOT_ELLIS_GC02M1B_MIPI_RAW [PhysEnumDevice:0xa7957880]
  Virtual Devices: # 4
    [device@3.6/internal/0] -> 00 torchModeStatus:AVAILABLE_OFF hasFlashUnit:1 [VirtEnumDevice:0xa794dbc0 IVirtualDevice:0xa7e0a690]
    [device@3.6/internal/1] -> 01 torchModeStatus:NOT_AVAILABLE hasFlashUnit:0 [VirtEnumDevice:0xa794dce0 IVirtualDevice:0xa7e0ab60]
    [device@3.6/internal/2] -> 02 torchModeStatus:NOT_AVAILABLE hasFlashUnit:0 [VirtEnumDevice:0xa794dd10 IVirtualDevice:0xa7e0abd0]
    [device@3.6/internal/3] -> 03 torchModeStatus:AVAILABLE_OFF hasFlashUnit:1 [VirtEnumDevice:0xa794ddd0 IVirtualDevice:0xa7e0ac40]
  Open Devices: # 0 (multi-opened maximum: # 1)

################################################################################
## 07-10 10:22:19.955 (1)
## ICameraDevice
## Camera device [0]
## Camera device [device@3.6/internal/0]

== state transition (most recent at bottom): Camera device ==
  07-10 10:22:19.701 : -> initialized

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  [no events yet]

== debug state (most recent at bottom): App Stream Manager ==
  [no events yet]

################################################################################
## 07-10 10:22:19.956 (1)
## ICameraDevice
## Camera device [1]
## Camera device [device@3.6/internal/1]

== state transition (most recent at bottom): Camera device ==
  07-10 10:22:19.760 : -> initialized

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  [no events yet]

== debug state (most recent at bottom): App Stream Manager ==
  [no events yet]

################################################################################
## 07-10 10:22:19.958 (1)
## ICameraDevice
## Camera device [2]
## Camera device [device@3.6/internal/2]

== state transition (most recent at bottom): Camera device ==
  07-10 10:22:19.820 : -> initialized

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  [no events yet]

== debug state (most recent at bottom): App Stream Manager ==
  [no events yet]

################################################################################
## 07-10 10:22:19.959 (1)
## ICameraDevice
## Camera device [3]
## Camera device [device@3.6/internal/3]

== state transition (most recent at bottom): Camera device ==
  07-10 10:22:19.938 : -> initialized

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  [no events yet]

== debug state (most recent at bottom): App Stream Manager ==
  [no events yet]

################################################################################
## 07-10 10:22:16.147 (0)
## NSCam::ULog
Dump time: 07-10 10:33:27.218054
Flushed!

################################################################################
## 07-10 10:22:20.106 (0)
## NSCam::v3::IStreamInfoPluginManager
Registered Plugin(s):
{ .pluginId=P1STT .options=1 .variantData<1> } [libmtkcam_streaminfo_plugin-p1stt.so 1:0xdba22e99]

################################################################################
## 07-10 10:22:16.146 (-1)
## debug
---
## Reporting done - (07-10 10:33:27.231)
